



How to Unlink the Z Cooler Walkway Automation Rev 0.00

You can unlink the automation of the Walkway if needed. If you have a walkway along the side of the cooler or, over the top of the cooler, or freestanding, ect. There can be many reasons to unlink the walkway. Here is how to unlink the model so you can use it in other ways as required for your job.

**Please do not unlink the walkway unless you really need to.**

Open the “WLK Part model” you need to unlink.

To unlink the length automation, edit the “Sketch Base”. Remove the equal on the yellow highlighted lines (=30 & =32). Then change the yellow highlighted dims to Driving. So they can manually be changed to your needs.

A diagram of a graph

AI-generated content may be incorrect.

A line with a green square and a green square

AI-generated content may be incorrect.

To unlink the mounting holes. Edit the sketch for the hole. Remove the equal on the yellow highlighted line (=6). Then change the yellow highlighted dim to Driving.

A blue rectangular object with green squares and numbers

AI-generated content may be incorrect.

A drawing of a wooden structure

AI-generated content may be incorrect.