



XCH Cooler Automation Rev 0.00

The XCH Master Cooler was released on 7-1-25.

Rev 0.01 – Fan Deck & Panel Support

The Fan Deck automation (FDK) has been updated. It has not been fully checked due to the Solid Works update on 10-3-25. So there may be more updates to follow.

The drop down for the fan size are unchanged. There is a new option for the full panels

(21240 & 21242) have an opinion of 24” & 18“. 24 is our standard.

A screenshot of a spreadsheet

AI-generated content may be incorrect.

The length & width of the FDK are both tied to the 3D Sketch in the ASM & will update when it is updated. I do suggest that if the fan is smaller than the master. Change the fan size before you update the ASM. If the fan is Bigger, I suggest you change the ASM first. Then update the FDK. This should keep the fan deck from messing up.

The FDK will now automatically update to the col size (W6 or W8).

The Panel Support (21210) is now automated as well to update to the col size (W6=3 or W8=4).

A blue and white metal frame

AI-generated content may be incorrect.