DO NOT USES THE 10” DESIGN PER R&D

USE 12” DESIGN

IT HAS LESS VIBRATION